SDRX.CONF Options
=================

Most options are initialized and maintained automatically and have corresponding GUI elements.
This file describes the ones that are only read.

audio.BassBufferTime
--------------------
Sets the [playback buffer](http://www.un4seen.com/doc/#bass/BASS_CONFIG_BUFFER.html) used by Bass.
Unit: Milliseconds
Default: 500

vfo.MinIFRate
-------------
Minimum Samplerate for first IF. This is the maximum demodulator bandwith.
Actual samplerate chosen may be higher than this, since the division factor from device rate is always
a power of two.
Unit: Hz
Default: 180000

vfo.IQBufferLen
---------------
Number of Samples in the incoming IQ buffer.
Unit: Samples
Default: 32768

vfo.IQProcBlock
--------------------
Sets the block of IQ data processed at once. Smaller blocks mean more overhead, larger blocks mean more
latency and may require larger buffers.
Unit: Milliseconds
Default: 50
